# AquifersMinor

Shapefile

Tags
subcrop, Texas, outcrop, TX, Minor aquifers, Aquifers, State of Texas

Summary
To update the delineations for the minor aquifers of Texas for the purpose of adding them to the 1991 Water Plan. This feature class is a component of TPWD 'base' data. 'Base' data includes current, statewide geospatial information intended to provide context for mapping purposes.

Description

This is a dataset containing what the Texas Water Development Board (TWDB) in Austin, Texas considers the 21 Minor aquifers of Texas.

Credits
There are no credits for this item.

Use limitations
This data was prepared for inclusion in the TPWD Base SDE database by the Texas Parks and Wildlife Department GIS Lab. The Texas Parks and Wildlife Department, its employees, and personnel, make no warranty as to its accuracy. The Texas Parks & Wildlife Department, its employees, and personnel MAKE NO WARRANTY FOR FITNESS OF USE FOR A PARTICULAR PURPOSE EXPRESS OR IMPLIED WITH RESPECT TO THIS DATA. THIS IS NOT A SURVEYED PRODUCT. Title 1 Part 10 Chapter 201 Rule §201.6 of the Texas Administrative Code suggests data showing the full extent of Texas be projected in the Texas State Mapping System. This feature class as provided by TPWD is unprojected.

## ArcGIS Metadata ▼►

## Topics and Keywords ▼►

Place keywordsTexas, TX, State of Texas

Theme keywordssubcrop, outcrop, Minor aquifers, Aquifers

Hide Topics and Keywords ▲

## Citation ▼►

* TitleAquifersMinor
Publication date1997-01-01
Presentation formats *digital map
Hide Citation ▲

## Resource Details ▼►

Dataset languagesEnglish (UNITED STATES)
Statuscompleted
Spatial representation type *vector
Supplemental information

      Lines were digitized from the Bureau of Economic Geology's Geologic Atlas Sheets (GAT) at 1:250,000 scale. Work started in January 1990 and was completed in May 1990. All digitizing was done at the USGS office in Austin, Texas using Arc/Info. The Yegua Jackson aquifer was digitized and added to the original dataset in 2001. REVISIONS MADE TO THE MINOR AQUIFERS FOR THE 2007 STATE WATER PLAN: The boundary of the Blaine aquifer was revised based on current information from well yields, groundwater levels, and groundwater chemistry. It was extended farther south to include most of the larger outcrops of the Blaine Formation. The boundaries of the Blaine Formation are based on the digital Geological Atlas of Texas (see TNRIS). The downdip extent of the aquifer, west of the exposure of the Blaine Formation, includes wells that produce groundwater with total dissolved solids of 10,000 ppm or less. The subsurface boundary along parts of the aquifer to the east includes all wells that draw water from the aquifer, and is not defined in terms of groundwater salinity. More information on the new aquifer boundary can be found in the Texas 2007 State Water plan at http://www.twdb.state.tx.us/home/index.asp. The Bone Springs–Victorio Peak aquifer is defined on the east by the center line of the Salt Basin, the original, pre-development discharge for groundwater flow in the area. Its southern boundary coincides with the Bitterwell Break, a Tertiary normal fault, out of the Salt Basin. This feature reportedly corresponds to a groundwater divide. Moving westward, the southern boundary transfers from the Bitterwell Break to the Babb Flexure, a structural hinge or bend in the rocks. To the northwest, the boundary follows a flow line based on the area’s potentiometric surface. The northern extent of the aquifer in Texas is defined by the state line with New Mexico. More information on the new aquifer boundary can be found in the Texas 2007 State Water plan at http://www.twdb.state.tx.us/home/index.asp. The revised boundary for the Igneous aquifer encloses contiguous Tertiary igneous rocks. Large exposures of pre-Tertiary, mainly Cretaceous, age rocks were kept outside of the boundary. It is defined to include the majority of wells drawing from Tertiary igneous rocks. For the most part, the boundary follows that defined by the USGS. However, the revised boundary excludes the northernmost extension of the USGS boundary in Culberson County since that area consists of mostly Permian rocks, and includes areas of Tertiary rocks that are within a LBG-Guyton boundary in the northeast part of the study area. We included an area in the southwest part of the proposed boundary because that area appears to contain Tertiary igneous rocks overlain by Quaternary sediments. More information on the new aquifer boundary can be found in the Texas 2007 State Water plan at http://www.twdb.state.tx.us/home/index.asp. The revised boundary for the Lipan aquifer includes Quaternary alluvium, mainly Qau, outside the present boundary. By including more alluvium the Lipan aquifer is coincident with the boundary for the Edwards-Trinity Plateau aquifer to the north, west, and south. To the east the boundary remains essentially unchanged, occurring at the boundary between the Leona Formation and the Permian Clear Fork Group or Lueders Formation. The boundary of the GAM model, defined by the groundwater divide, is used to determine a subsurface limit for the Lipan aquifer to the south. The northern edge of the Edwards-Trinity Plateau aquifer defines the northern subsurface boundary. The contact between the Permian Clear Fork Group and the Lueders Formation is extended along strike to the south to delineate an eastern subsurface limit. More information on the new aquifer boundary can be found in the Texas 2007 State Water plan at http://www.twdb.state.tx.us/home/index.asp. Minor adjustments to the eastern boundary of the 'Presidio-Redford' portion of the West Texas Bolsons aquifer were done to show the contact with the new Igneous aquifer boundary. Minor adjustments were also made to show the contact with a smaller portion of the 'bolsons'/Igneous boundary in western Jeff Davis and southern Culberson county. (Editing was done in ArcGIS 9.1) Original contact information for this dataset: Mark Hayes TWDB mailing and physical address: 1700 North Congress Avenue PO Box 13231 Austin, Texas 78711-3231 USA (512)936-0828 (voice) (512)463-8423 (fax) mark.hayes@twdb.state.tx.us

* Processing environmentMicrosoft Windows XP Version 5.1 (Build 2600) Service Pack 3; ESRI ArcGIS 10.0.3.3600
ArcGIS item properties

* NameAquifersMinor
* Size10.015
* Locationfile://\\GIS-CBANKSXP\E\PDaugherty\data\Data_Downloads\AquifersMinor.shp

* Access protocolLocal Area Network

* Content typeDownloadable Data

Hide Resource Details ▲

## Extents ▼►

Extent

Geographic extent

Bounding rectangle

Extent typeExtent used for searching
* West longitude-105.849205
* East longitude-93.609390
* North latitude36.501232
* South latitude26.352266
* Extent contains the resourceYes

Extent in the item's coordinate system

* West longitude-105.849205
* East longitude-93.609390
* South latitude26.352266
* North latitude36.501232
* Extent contains the resourceYes

Hide Extents ▲

## Resource Points of Contact ▼►

Point of contact

Organization's nameTexas Parks and Wildlife Department GIS Lab
Contact's rolepoint of contact

Contact information ▼►

Phone

Voice512-389-8070
Fax512-389-8300

Address

Typeboth
Delivery point4200 Smith School Road
CityAustin
Administrative areaTX
Postal code78744-3292
CountryUS
e-mail address mailto:gislab@tpwd.state.tx.us?subject=AquifersMinor

Hours of service8 am - 5 pm, Mon - Fri

Hide Contact information ▲

Hide Resource Points of Contact ▲

## Resource Maintenance ▼►

Resource maintenance

Update frequencyas needed

Hide Resource Maintenance ▲

## Resource Constraints ▼►

Constraints

Limitations of use

      This data was prepared for inclusion in the TPWD Base SDE database by the Texas Parks and Wildlife Department GIS Lab. The Texas Parks and Wildlife Department, its employees, and personnel, make no warranty as to its accuracy. The Texas Parks & Wildlife Department, its employees, and personnel MAKE NO WARRANTY FOR FITNESS OF USE FOR A PARTICULAR PURPOSE EXPRESS OR IMPLIED WITH RESPECT TO THIS DATA. THIS IS NOT A SURVEYED PRODUCT. Title 1 Part 10 Chapter 201 Rule §201.6 of the Texas Administrative Code suggests data showing the full extent of Texas be projected in the Texas State Mapping System. This feature class as provided by TPWD is unprojected.

Hide Resource Constraints ▲

## Spatial Reference ▼►

ArcGIS coordinate system

* TypeGeographic
* Geographic coordinate referenceGCS_North_American_1983
* Coordinate reference details

Geographic coordinate system

Well-known identifier4269
X origin-399.99999999999989
Y origin-399.99999999999989
XY scale11258999068426.24
Z origin-100000
Z scale10000
M origin-100000
M scale10000
XY tolerance8.9831528411952117e-009
Z tolerance0.001
M tolerance0.001
High precisiontrue
Left longitude-180
Well-known textGEOGCS["GCS_North_American_1983",DATUM["D_North_American_1983",SPHEROID["GRS_1980",6378137.0,298.257222101]],PRIMEM["Greenwich",0.0],UNIT["Degree",0.0174532925199433],AUTHORITY["EPSG",4269]]

Reference system identifier

* Value4269
* CodespaceEPSG
* Version7.4.1

Hide Spatial Reference ▲

## Spatial Data Properties ▼►

Vector ▼►

* Level of topology for this datasetgeometry only
Geometric objects

Feature class nameAquifersMinor
* Object typecomposite
* Object count538

Hide Vector ▲
ArcGIS Feature Class Properties ▼►

* Feature typeSimple
* Geometry typePolygon
* Has topologyFALSE
* Feature count538
* Spatial indexTRUE
* Linear referencingFALSE

Hide ArcGIS Feature Class Properties ▲
Hide Spatial Data Properties ▲

## Data Quality ▼►

Scope of quality information ▼►

Resource leveldataset

Hide Scope of quality information ▲
Hide Data Quality ▲

## Distribution ▼►

Distributor ▼►

Contact information

Individual's nameMarian O'Brien
Organization's nameTexas Parks and Wildlife Department
Contact's positionGIS Analyst
Contact's roledistributor

Contact information ▼►

Phone

Voice512-389-8315
Fax512-389-8300

Address

Typeboth
Delivery point4200 Smith School Road
CityAustin
Administrative areaTX
Postal code78744-3292
CountryUS
e-mail address mailto:marian.obrien@tpwd.state.tx.us?subject=AquifersMinor

Hours of service8 am - 5 pm, Mon - Fri

Hide Contact information ▲

Hide Distributor ▲
Distribution format

* Format nameShapefile

Transfer options

* Transfer size10.015

Hide Distribution ▲

## Fields and Subtypes ▼►

Details for object AquifersMinor ▼►

* TypeFeature Class
* Row count538
Field FID ▼►

* AliasFID
* Data typeOID
* Width4
* Precision0
* Scale0
* Field description

      Internal feature number.

* Description source

      ESRI

* Description of valuesSequential unique whole numbers that are automatically generated.

Hide Field FID ▲
Field Shape ▼►

* AliasShape
* Data typeGeometry
* Width0
* Precision0
* Scale0
* Field description

      Feature geometry.

* Description source

      ESRI

Description of valuesCoordinates defining the features.

Hide Field Shape ▲
Field Name ▼►

* AliasName
* Data typeString
* Width30
* Precision0
* Scale0
Field description

      Aquifer Name

Description source

      TWDB

Hide Field Name ▲
Field Code ▼►

* AliasCode
* Data typeString
* Width2
* Precision0
* Scale0
Field description

      The number '0' refers to a hole in the aquifer (no outcrop or subcrop/downdip). The number '1' refers to the outcrop (at the surface). The number '2', refers to the subcrop or downdip (below the surface).

Description source

      TWDB

Hide Field Code ▲
Field SqMiCalc ▼►

* AliasSqMiCalc
* Data typeDouble
* Width19
* Precision0
* Scale0
Field description

      Area in square miles

Description source

      Calculated in GIS using Texas Centric Albers Equal Area Projection

Hide Field SqMiCalc ▲
Field AcresCalc ▼►

* AliasAcresCalc
* Data typeDouble
* Width19
* Precision0
* Scale0
Field description

      Area in acres

Description source

      Calculated in GIS using Texas Centric Albers Equal Area Projection

Hide Field AcresCalc ▲
Field Shape_Leng ▼►

* AliasShape_Leng
* Data typeDouble
* Width19
* Precision0
* Scale0

Hide Field Shape_Leng ▲
Field Shape_Area ▼►

* AliasShape_Area
* Data typeDouble
* Width19
* Precision0
* Scale0
* Field description

      Area of feature in internal units squared.

* Description source

      ESRI

* Description of valuesPositive real numbers that are automatically generated.

Hide Field Shape_Area ▲

Hide Details for object AquifersMinor ▲
Hide Fields and Subtypes ▲

## Metadata Details ▼►

Metadata languageEnglish (UNITED STATES)
Scope of the data described by the metadatadataset
Scope name *dataset
* Last update2012-11-09
ArcGIS metadata properties

Metadata formatArcGIS 1.0
Standard or profile used to edit metadataNAP
Created in ArcGIS2010-05-17T10:27:40
Last modified in ArcGIS2012-11-09T10:48:21
Automatic updates

Have been performedYes
Last update2012-11-09T10:48:21

Hide Metadata Details ▲

## Metadata Contacts ▼►

Metadata contact

Organization's nameTexas Parks and Wildlife Department
Contact's rolepoint of contact

Contact information ▼►

Phone

Voice512-389-8070
Fax512-389-8300

Address

Typeboth
Delivery point4200 Smith School Road
CityAustin
Administrative areaTX
Postal code78744-3292
CountryUS
e-mail address mailto:gislab@tpwd.state.tx.us?subject=AquifersMinor

Hours of service8 am - 5 pm, Mon - Fri

Hide Contact information ▲

Hide Metadata Contacts ▲

## Metadata Constraints ▼►

Security constraints

Classificationunclassified

Hide Metadata Constraints ▲

## Thumbnail and Enclosures ▼►

Thumbnail

Thumbnail typeJPG

Enclosure

Enclosure typeFile
Description of enclosureoriginal metadata
Original metadata document, which was translatedyes
Original file namesource_metadata.xml

Hide Thumbnail and Enclosures ▲

## FGDC Metadata (read-only) ▼►

## Identification ▼►

  Citation
    Citation Information
      Publication Date 1997
      Title
        Base.HYDRO.AquifersMinor
      Geospatial Data Presentation Form vector digital data
      Online Linkage Service=sde:sqlserver:GIS-DBBETA\tpwd_gisdev; Database=Base; User=Hydro; Version=sde.DEFAULT
  Description
    Abstract

          This is a dataset containing what the Texas Water Development Board (TWDB) in Austin, Texas considers the 21 Minor aquifers of Texas.

    Purpose

          To update the delineations for the minor aquifers of Texas for the purpose of adding them to the 1991 Water Plan.

          This feature class is a component of TPWD 'base' data.
          'Base' data includes current, statewide geospatial information intended to provide context for mapping purposes.

    Supplemental Information

          Lines were digitized from the Bureau of Economic Geology's Geologic Atlas Sheets (GAT) at 1:250,000 scale.   Work started in January 1990 and was completed in May 1990. All digitizing was done at the USGS office in Austin, Texas using Arc/Info.
          The Yegua Jackson aquifer was digitized and added to the original dataset in 2001.

          REVISIONS MADE TO THE MINOR AQUIFERS FOR THE 2007 STATE WATER PLAN:  The boundary of the Blaine aquifer was revised based on current information from well yields, groundwater levels, and groundwater chemistry. It was extended farther south to include most of the larger outcrops of the Blaine Formation. The boundaries of the Blaine Formation are based on the digital Geological Atlas of Texas (see TNRIS). The downdip extent of the aquifer, west of the exposure of the Blaine Formation, includes wells that produce groundwater with total dissolved solids of 10,000 ppm or less. The subsurface boundary along parts of the aquifer to the east includes all wells that draw water from the aquifer, and is not defined in terms of groundwater salinity. More information on the new aquifer boundary can be found in the Texas 2007 State Water plan at http://www.twdb.state.tx.us/home/index.asp.
          The Bone Springs–Victorio Peak aquifer is defined on the east by the center line of the Salt Basin, the original, pre-development discharge for groundwater flow in the area. Its southern boundary coincides with the Bitterwell Break, a Tertiary normal fault, out of the Salt Basin. This feature reportedly corresponds to a groundwater divide. Moving westward, the southern boundary transfers from the Bitterwell Break to the Babb Flexure, a structural hinge or bend in the rocks. To the northwest, the boundary follows a flow line based on the area’s potentiometric surface. The northern extent of the aquifer in Texas is defined by the state line with New Mexico. More information on the new aquifer boundary can be found in the Texas 2007 State Water plan at http://www.twdb.state.tx.us/home/index.asp.
          The revised boundary for the Igneous aquifer encloses contiguous Tertiary igneous rocks. Large exposures of pre-Tertiary, mainly Cretaceous, age rocks were kept outside of the boundary. It is defined to include the majority of wells drawing from Tertiary igneous rocks. For the most part, the boundary follows that defined by the USGS. However, the revised boundary excludes the northernmost extension of the USGS boundary in Culberson County since that area consists of mostly Permian rocks, and includes areas of Tertiary rocks that are within a LBG-Guyton boundary in the northeast part of the study area. We included an area in the southwest part of the proposed boundary because that area appears to contain Tertiary igneous rocks overlain by Quaternary sediments. More information on the new aquifer boundary can be found in the Texas 2007 State Water plan at http://www.twdb.state.tx.us/home/index.asp.
          The revised boundary for the Lipan aquifer includes Quaternary alluvium, mainly Qau, outside the present boundary. By including more alluvium the Lipan aquifer is coincident with the boundary for the Edwards-Trinity Plateau aquifer to the north, west, and south. To the east the boundary remains essentially unchanged, occurring at the boundary between the Leona Formation and the Permian Clear Fork Group or Lueders Formation. The boundary of the GAM model, defined by the groundwater divide, is used to determine a subsurface limit for the Lipan aquifer to the south. The northern edge of the Edwards-Trinity Plateau aquifer defines the northern subsurface boundary. The contact between the Permian Clear Fork Group and the Lueders Formation is extended along strike to the south to delineate an eastern subsurface limit. More information on the new aquifer boundary can be found in the Texas 2007 State Water plan at http://www.twdb.state.tx.us/home/index.asp.
          Minor adjustments to the eastern boundary of the 'Presidio-Redford' portion of the West Texas Bolsons aquifer were done to show the contact with the new Igneous aquifer boundary.
          Minor adjustments were also made to show the contact with a smaller portion of the 'bolsons'/Igneous boundary in western Jeff Davis and southern Culberson county.
          (Editing was done in ArcGIS 9.1)

          Original contact information for this dataset:

          Mark Hayes
          TWDB
          mailing and physical address:

          1700 North Congress Avenue
          PO Box 13231
          Austin, Texas 78711-3231
          USA

          (512)936-0828 (voice)
          (512)463-8423 (fax)
          mark.hayes@twdb.state.tx.us

  Time Period of Content
    Time Period Information
      Multiple Dates/Times
        Single Date/Time
          Calendar Date Geometry: 1997
        Single Date/Time
          Calendar Date Attributes: 05/17/2010
    Currentness Reference

          publication date

  Status
    Progress Complete
    Maintenance and Update Frequency As needed
  Spatial Domain
    Bounding Coordinates
      West Bounding Coordinate -105.849205
      East Bounding Coordinate -93.609390
      North Bounding Coordinate 36.501232
      South Bounding Coordinate 26.352266
  Keywords
    Theme
      Theme Keyword Aquifers
      Theme Keyword Minor aquifers
      Theme Keyword outcrop
      Theme Keyword subcrop
    Place
      Place Keyword Texas
      Place Keyword TX
      Place Keyword State of Texas
  Access Constraints

        None.

  Use Constraints

        This data was prepared for inclusion in the TPWD Base SDE database by the Texas Parks and Wildlife Department GIS Lab.  The Texas Parks and Wildlife Department, its employees, and personnel, make no warranty as to its accuracy. The Texas Parks & Wildlife Department, its employees, and personnel MAKE NO WARRANTY FOR FITNESS OF USE FOR A PARTICULAR PURPOSE EXPRESS OR IMPLIED WITH RESPECT TO THIS DATA. THIS IS NOT A SURVEYED PRODUCT.

        Title 1 Part 10 Chapter 201 Rule §201.6 of the Texas Administrative Code suggests data showing the full extent of Texas be projected in the Texas State Mapping System. This feature class as provided by TPWD is unprojected.

  Point of Contact
    Contact Information
      Contact Organization Primary
        Contact Organization Texas Parks and Wildlife Department GIS Lab
      Contact Address
        Address Type mailing and physical address
        Address 4200 Smith School Road
        City Austin
        State or Province TX
        Postal Code 78744-3292
        Country UNITED STATES
      Contact Voice Telephone 512-389-8070
      Contact Facsimile Telephone 512-389-8300
      Contact Electronic Mail Address mailto:gislab@tpwd.state.tx.us?subject=AquifersMinor
      Hours of Service 8 am - 5 pm, Mon - Fri
  Native Data Set Environment
    Microsoft Windows XP Version 5.1 (Build 2600) Service Pack 3; ESRI ArcCatalog 9.3.1.3000

Hide Identification ▲

## Data Quality ▼►

  Lineage
    Process Step
      Process Description

            Dataset copied.

      Process Date 20100122 16021600
    Process Step
      Process Description

            Dataset copied.

      Source Used Citation Abbreviation
        \\Gis-datasrvr\Gis_Data\GIS_Shared\EnterpriseGIS_Workgroup\counties
      Process Date 20100122 16041700
    Process Step
      Process Description

            Dataset copied.

      Process Date 20100205 09083300
    Process Step
      Process Description

            Dataset copied.

      Source Used Citation Abbreviation
        W:\GIS_Shared\EnterpriseGIS_Workgroup\DataLayersList\OfficialShape\County
      Process Date 2010-02-11
      Process Time 11144300
    Process Step
      Process Description

            Metadata imported.

      Source Used Citation Abbreviation
        M:\EnterpriseGIS_Workgroup\DataLayersList\Metadata\BaseMetadataTemplate.xml
      Process Date 2010-05-17
      Process Time 10193400
    Process Step
      Process Description

            Dataset copied.

      Source Used Citation Abbreviation
        \\Gis-datasrvr\GIS_Shared\EnterpriseGIS_Workgroup\DataLayersList\shp\Aquifers\AquiferMinor
      Process Date 2010-05-17
      Process Time 10274000

Hide Data Quality ▲

## Spatial Reference ▼►

  Horizontal Coordinate System Definition
    Geographic
      Latitude Resolution 0.000000
      Longitude Resolution 0.000000
      Geographic Coordinate Units Decimal degrees
    Geodetic Model
      Horizontal Datum Name North American Datum of 1983
      Ellipsoid Name Geodetic Reference System 80
      Semi-major Axis 6378137.000000
      Denominator of Flattening Ratio 298.257222
  Vertical Coordinate System Definition
    Altitude System Definition
      Altitude Resolution 1.000000
      Altitude Encoding Method Explicit elevation coordinate included with horizontal coordinates

Hide Spatial Reference ▲

## Entities and Attributes ▼►

  Detailed Description
    Entity Type
      Entity Type Label AquifersMinor
    Attribute
      Attribute Label FID
      Attribute Definition
        Internal feature number.
      Attribute Definition Source ESRI
      Attribute Domain Values
        Unrepresentable Domain
          Sequential unique whole numbers that are automatically generated.
    Attribute
      Attribute Label Shape
      Attribute Definition
        Feature geometry.
      Attribute Definition Source ESRI
      Attribute Domain Values
        Unrepresentable Domain
          Coordinates defining the features.
    Attribute
      Attribute Label Name
      Attribute Definition
        Aquifer Name
      Attribute Definition Source TWDB
    Attribute
      Attribute Label Code
      Attribute Definition
        The number '0' refers to a hole in the aquifer (no outcrop or subcrop/downdip). The number '1' refers to the outcrop (at the surface). The number '2', refers to the subcrop or downdip (below the surface).
      Attribute Definition Source TWDB
    Attribute
      Attribute Label SqMiCalc
      Attribute Definition
        Area in square miles
      Attribute Definition Source Calculated in GIS using Texas Centric Albers Equal Area Projection
    Attribute
      Attribute Label AcresCalc
      Attribute Definition
        Area in acres
      Attribute Definition Source Calculated in GIS using Texas Centric Albers Equal Area Projection
    Attribute
      Attribute Label Shape_Leng
    Attribute
      Attribute Label Shape_Area
      Attribute Definition
        Area of feature in internal units squared.
      Attribute Definition Source ESRI
      Attribute Domain Values
        Unrepresentable Domain
          Positive real numbers that are automatically generated.

Hide Entities and Attributes ▲

## Distribution Information ▼►

  Distributor
    Contact Information
      Contact Organization Primary
        Contact Organization Texas Parks and Wildlife Department
        Contact Person Cynthia R. Banks
      Contact Position GIS Data Librarian
      Contact Address
        Address Type mailing and physical address
        Address 4200 Smith School Road
        City Austin
        State or Province TX
        Postal Code 78744-3292
        Country UNITED STATES
      Contact Voice Telephone 512-389-8073
      Contact Facsimile Telephone 512-389-8300
      Contact Electronic Mail Address mailto:cynthia.banks@tpwd.state.tx.us?subject=AquifersMinor
      Hours of Service 8 am - 5 pm, Mon - Fri
  Resource Description Downloadable Data
  Standard Order Process
    Digital Form
      Digital Transfer Information
        Transfer Size 3.104

Hide Distribution Information ▲

## Metadata Reference ▼►

  Metadata Date 2010-12-10
  Metadata Contact
    Contact Information
      Contact Organization Primary
        Contact Organization Texas Parks and Wildlife Department
      Contact Address
        Address Type mailing and physical address
        Address 4200 Smith School Road
        City Austin
        State or Province TX
        Postal Code 78744-3292
        Country UNITED STATES
      Contact Voice Telephone 512-389-8070
      Contact Facsimile Telephone 512-389-8300
      Contact Electronic Mail Address mailto:gislab@tpwd.state.tx.us?subject=AquifersMinor
      Hours of Service 8 am - 5 pm, Mon - Fri
  Metadata Standard Name FGDC Content Standards for Digital Geospatial Metadata
  Metadata Standard Version FGDC-STD-001-1998
  Metadata Time Convention local time
  Metadata Access Constraints None
  Metadata Use Constraints
    None
  Metadata Security Information
    Metadata Security Classification Unclassified
  Metadata Extensions
    Online Linkage http://www.esri.com/metadata/esriprof80.html
    Profile Name ESRI Metadata Profile

Hide Metadata Reference ▲