Data: 2015 TPWD West Galveston Bay and Christmas Bay Seagrass Extent

Production year: 2015

Method: Photointerpretation; Seagrass presence/absence was manually delineated from 0.1-m aerial imagery

MMU: 100 m2

Datum and Projection: NAD83 UTM 15N

Imagery Source: The digital orthophotography and color infrared digital orthos composed of 24 bit natural color and color infrared digital orthos at a scale of 1 to 840 with a 0.10 meter pixel resolution. Imagery acquired on February 9, 2015.

Note: The imagery boundary did not include ALL of West Galveston Bay; see data boundary for mapping extent.

Accuracy Assessment: Ground-truthing conducted with accuracy greater than 80%.